Data underlying the paper: Thermodynamics and kinetics of moisture transport in bitumen

Authors: L Ma, A Varveri, R Jing, S Erkens
TU Delft, Faculty of Civil Engineering and Geosciences, Department of Engineering Structures.

Faculty of Civil Engineering & Geosciences
Section of Pavement Engineering
Stevinweg 1
2628 CN, Delft
The Netherlands
Room: Stevin II 1.26

-------------------------------------
This dataset contains data collected for the investigation of moisture diffusion in bitumen.

It is being made public both to act as supplementary data for publications and the PhD thesis of Lili Ma and in order for other researchers to use this data in their own work.

The data in this data set was collected in the Pavement Engineering Laboratory of the Delft University of Technology between 2019 and 2020.

This research project was made possible by a grant from the China Scholarship Council (CSC).

-------------------------------------
All the results were performed in the equipment Dynamic vapor sorption. Detailed settings of drying methods, testing temperatures, and relative humidity can be obtained in the raw files.

For each file, V710, T710, and VPMB represent different bituminous binders. "80%" is the measuring relative humidity. "C" denotes temperature. Files start with "1" involve results measured at relative humidity ranging from 0 to 100% with a step of 10%. 

For details regarding post processing and analysis, readers are referred to the paper "Thermodynamics and kinetics of moisture transport in bitumen".

For more questions, please contact Lili Ma (lili.ma@tudelft.nl).