Data underlying the publication: The Mechanism behind Vibration Assisted Fluidization of Cohesive Micro-Silica

Dataset contains the raw data of:
	-	Pressure drop measurements
		Equipment: OMEGA PX409-10WG5V
		Comments:  Bed pressure drop as measured at various superficial gas velocities in the presence and absence of mechanical vibration, normalized by static pressure
		Output:	   Normalized pressure drop (-) vs superficial gas velocity (cm/s)

	-	Particle size distribution (primary particles)
		Equipment: Malvern 3000
		Comments:  Performed at 4 bar acceleration, equipped with high energy ventury
		Output:	   Particle size distribution; particle size (um), probability density (1/um), cumulative (%)

	-	Particle size distribution (agglomerates)
		Equipment: Zeiss Colibri 7 Axio Observer microscope, equipped with Orca Flash 4.0 Hamamatsu V2 camera
		Comments:  Images were analysed to measure agglomerate sizes using Fiji (ImageJ)
		Output:    Size distributions; particle d_10, d_50 and d_90 are reported (um)

	-	Xray images
		Equipment: Source: Yxlon International GmbH, with amaximum energy of 150 keV working in cone beam mode
		           Detector: Teledyne Dalsa Xineos
 		Comments:  30.000 images were shot per experiment (600s x 50Hz), the selected images as put in the manuscript are included	
                           Images were attained by processing the aquired data as described in the manuscript, processing was performed in MatLab 
		Output:    X-ray images (-)