Figure 6. Dynamic response of microgel layer to pH
The MEM is immersen in solution of pH 6.5 and 3.0 and the first measurement of the thickness starts at t = 10min.
Every 8 minutes a new image is being taken of the same region of the MEM. The thickness in different regions is being estimated
and an average value is being calculated.