Files explanation

Electrosurgery-continues-blend mode-40W.wmv: a recoding of thermal camera during
electrosurgery on porcine tissue for 1 minutes continuously in blend mode and 40 W power
using the electrosurgical knife. 

Electrosurgery-continus-fulgurate-40W.wmv : a recoding of thermal camera during
electrosurgery on porcine tissue for 1 minutes continuously in fulgurate-mode and 40 W power
using the electrosurgical knife. 

Electrosurgery-continus-spray-40W.wmv:  a recoding of thermal camera during
electrosurgery on porcine tissue for 1 minutes continuously in spray-mode and 40 W power
using the electrosurgical knife. 

Max temperature during electrosurgery.docx: an microsoft word file that contains a table
reporting the max temperature that the blade of the electrosurgical reached durig the electrosurgery 
of the porcine tissue in different setting (different powers of 40, 50 and 60 W, different mode
of blend, spray, fulguration). These data is illustrated in the paper (10.1109/TBME.2024.3362235) in figure 3.