 General overview
●        Name: 3D models for studying the effect of slicing on the properties of metallic copper in additive electrochemical manufacturing (ECAM)
●        Creator: Babchuk, Roman; Vasyliev, Georgii. National Technical University of Ukraine “Igor Sikorsky Kyiv Polytechnic Institute”, 37, Prospect Beresteiskyi, Kyiv-56 03056, Ukraine
●        Identifier: CTZ124
●        Date: project start 2025-01-01; project end 2027-12-31; release date 2025-06-24
●        Method: Software “Blender” for creating models in “.stl” format. Ultimaker Cura for converting ".stl” files into “.gcode”.
●        Processing: .gcode files processing in .txt format (Notepad). Created by Ultimaker Cura from models in .STL format. STL files created by Blender. 
●        Funder: Ministry of Education and Science of Ukraine (Reg. number 0125U000705, 2025)
Content description
●        Topic: additive manufacturing; ECAM; G-code; slicing.
●        Language: English.
●        Code List: Cons - means concentric infill; Zigzag - means zigzag infill; Triangle - means triangle infill; 1, 2, 4 mm - means inflill line distance of 1, 2, 4 mm, correspondingly.
Technical description
●        File inventory: G-code.rar
●        File formats:  .GCODE
●        File structure: separate files for different infill parameters and different step values. 
●        Version: 1.0
●        Required software: Ultimaker Cura.
Access
●        Rights: CC-BY
●        Access information:
https://doi.org/10.4121/c4479e26-f9f8-4b25-b01a-100ef451a36c.v1